# ATEX VALIDATION TEST PROCEDURE

## VAP100B – Goods Inwards

### Data entry

1. No of PCBs - Anything less than 1 the window should close
2. Delivery date – should be in dd/mm/yy format
   1. Else – invalid syntax error should appear and restart the process
3. PON should be numerical values only and up to 8 characters
   1. Else – window should reappear prompting to re-enter correct value or click close to exit the program
4. CoC should also be numerical values up to 8 characters long
   1. Else – window should reappear prompting to re-enter correct value or click close to exit the program